Subcontractor´s certificate – Adhesives

Certificate refers to component/product:

|  |
| --- |
| *Click to fill****.***  |

## **2.1      Mandatory material requirements**

|  |
| --- |
| 2.1.1     SVHC/ECHA’s candidate list |
| No chemical substances listed on ECHA's candidate list of SVHC substances may occur in concentrations above 0.1% by weight, see <https://echa.europa.eu/candidate-list-table>0.1% by weight refers to chemical products or articles that are included or used in the manufacture of the furniture/product (i.e. each individual part of an item), not 0.1% of an assembled piece of furniture, see guidance document here: <https://echa.europa.eu/documents/10162/2324906/articles_en.pdf> |
| Does the product meet the above requirements? | Yes[ ]  | No[ ]  | Not relevant[ ]  |

### 2.1.8     Adhesives

|  |
| --- |
| 2.1.8.1 Adhesives |
| Adhesives that are used for the production of the piece of furniture or its components must contain less than 10% VOC (vapour pressure > 0,01kPa\*) by weight and also contain less than 0.2% free formaldehyde by weight.  The requirement applies to the glue itself without hardener. A valid safety data sheet (SDS), certificate from supplier or similar for all used adhesives must be available.The requirement of free formaldehyde is not valid for adhesives/binding agents used for production of particle boards, fibre boards (MDF, HDF), OSB, plywood and edge glued panels provided the emission of formaldehyde is less than as stated in section 2.1.2.2 “Formaldehyde in wood-based flat panels”. *\* According to regulation 2010/75/EU (Industrial Emissions Directive)* |
| Does the product meet the above requirements? | Yes[ ]  | No[ ]  | Not relevant[ ]  |

**This certifies that the component/product to which the certificate relates meets the above requirements according to Möbelfakta's requirement specification ver 2023-04-01 ver 15.**

**Supplier**: Click here

**Place**: Click here

**Date**: Click here

**Signature**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Print name**: Click here